general information

This Datalogger provides a services for external conenction. Here you'll have a Web Interface, SSH connection and a useable REST API.

WLAN connection

SSID

By default the SSID is myCar.

WPA-PSK TKIP Key

The key is: myCar1234