abstract

The filesystem is mounted readonly to prevent damages due to poweroff and poweron. But there is a synchronous mounted Filesystem with a robust filesystem under /mnt/myCar which holds the variable data captured during operation.

Filesystem paths

application stack

The software could be found unter /opt/myCar. Additional there are some symlinks pointing to the correct destinations.

Datarecording

/mnt/myCar/rec

configuration

/mnt/myCar/etc

Logfiles

/mnt/myCar/log