Intro

Diese Informationen stammen im wesentlichen aus Wikipedia. Für diesen Artikel sind nur offizielle Kanäle für Europa interessant

Kanäle

20 MHz Kanäle

add name=5GHZ#CH32 frequency=5160 comment=U-NII-1 skip-dfs-channels=all
add name=5GHZ#CH36 frequency=5180 comment=U-NII-1 skip-dfs-channels=all
add name=5GHZ#CH40 frequency=5200 comment=U-NII-1 skip-dfs-channels=all
add name=5GHZ#CH44 frequency=5220 comment=U-NII-1 skip-dfs-channels=all
add name=5GHZ#CH48 frequency=5240 comment=U-NII-1 skip-dfs-channels=all
add name=5GHZ#CH52 frequency=5260 comment=U-NII-2A skip-dfs-channels=disabled
add name=5GHZ#CH56 frequency=5280 comment=U-NII-2A skip-dfs-channels=disabled
add name=5GHZ#CH60 frequency=5300 comment=U-NII-2A skip-dfs-channels=disabled
add name=5GHZ#CH64 frequency=5320 comment=U-NII-2A skip-dfs-channels=disabled
add name=5GHZ#CH68 frequency=5340 comment=U-NII-2A skip-dfs-channels=disabled
add name=5GHZ#CH72 frequency=5360 comment=U-NII-2B skip-dfs-channels=all
add name=5GHZ#CH76 frequency=5380 comment=U-NII-2B skip-dfs-channels=all
add name=5GHZ#CH80 frequency=5400 comment=U-NII-2B skip-dfs-channels=all
add name=5GHZ#CH84 frequency=5420 comment=U-NII-2B skip-dfs-channels=all
add name=5GHZ#CH88 frequency=5440 comment=U-NII-2B skip-dfs-channels=all
add name=5GHZ#CH92 frequency=5460 comment=U-NII-2B skip-dfs-channels=all
add name=5GHZ#CH96 frequency=5480 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH100 frequency=5500 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH104 frequency=5520 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH108 frequency=5540 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH112 frequency=5560 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH116 frequency=5580 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH120 frequency=5600 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH124 frequency=5620 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH128 frequency=5640 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH132 frequency=5660 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH136 frequency=5680 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH140 frequency=5700 comment=U-NII-2C skip-dfs-channels=disabled
add name=5GHZ#CH144 frequency=5720 comment=U-NII-2C/3 skip-dfs-channels=all
add name=5GHZ#CH149 frequency=5745 comment=U-NII-3 skip-dfs-channels=all
add name=5GHZ#CH153 frequency=5765 comment=U-NII-3 skip-dfs-channels=all
add name=5GHZ#CH157 frequency=5785 comment=U-NII-3 skip-dfs-channels=all
add name=5GHZ#CH161 frequency=5805 comment=U-NII-3 skip-dfs-channels=all
add name=5GHZ#CH165 frequency=5825 comment=U-NII-3 skip-dfs-channels=all
add name=5GHZ#CH169 frequency=5845 comment=U-NII-3/4 skip-dfs-channels=all
add name=5GHZ#CH173 frequency=5865 comment=U-NII-4 skip-dfs-channels=all
add name=5GHZ#CH177 frequency=5885 comment=U-NII-4 skip-dfs-channels=all
add name=5GHZ#ALL20 frequency= 5160,5180,5200,5220,5240,5260,5280,5300,5320,5340,5360,5380,5400,5420,5440,5460,5480,5500,5520,5540,5560,5580,5600,5620,5640,5660,5680,5700,5720,5745,5765,5785,5805,5825,5845,5865,5885 skip-dfs-channels=disabled

40 MHz Kanäle

80 MHz Kanäle